GG0110Z

Item Summary | Previous item | Next item

Property | Specification
Data System

IRF-PAI
Data Specs V5.00.0 DRAFT
Description Prior Device - None of the above
XML Tag GG0110Z
Group Asmt
Type Checklist
Length 1
Fixed Start-End 1471-1471
Version Notes

Item Values
Value | LOINC | Text
0 |  | Not checked (No)
1 |  | Checked (Yes)
- |  | Not Asessed/No Information

Item Edits
Edit ID | Type | Severity | Edit Text
-5060 | Consistency | Fatal | GG0110 Consistency: a) If GG0110Z=[1], then all items from GG0110A through GG0110E must be equal to [0]. b) If GG0110Z=[0], then at least one of the items GG0110A through GG0110E must be equal to [1]. c) If GG0110Z=[-], then at least one item from GG0110A through GG0110E must equal [-], and all remaining items must equal [0,-].
-1010 | Format | Fatal | Invalid Data Value: The submitted value for this item is not in the valid range of acceptable values.

Item Summary | Previous item | Next item

NOTICE: These materials are in the public domain and cannot be copyrighted.
Generated: 03/16/2020 09:31:12 AM