-5133

Edit Summary | Previous edit | Next edit

Property | Specification
Data System

IRF-PAI
Data Specs V5.00.0 DRAFT
Edit Type Consistency
Severity Fatal
Edit Text (a) If O0110O1a = [0], then all active items from O0110O2a through O0110O4a must equal [0]
(b) If O0110O1a = [1], then at least one active item from O0110O2a through O0110O4a must not equal [0]
(c) If O0110O1a = [-], then all active items from O0110O2a through O0110O4a must equal [-]
Version Notes [V5.00.0] - Added new edit.

Item List
Item ID | Description
O0110O1a | Other: IV Access (Admission)
O0110O2a | Other: Peripheral (Admission)
O0110O3a | Other: Midline (Admission)
O0110O4a | Other: Central (Admission)

Edit Summary | Previous edit | Next edit

NOTICE: These materials are in the public domain and cannot be copyrighted.
Generated: 03/16/2020 09:31:12 AM