-5065

Edit Summary | Previous edit | Next edit

Property | Specification
Data System

IRF-PAI
Data Specs V5.00.0 DRAFT
Edit Type Consistency
Severity Fatal
Edit Text a) If GG0170Q1=[0], then items GG0170R1, GG0170R2, G0170RR1, GG0170S1, GG0170S2, and GG0170SS1 must be equal to [^].
b) If GG0170Q1=[1], then items GG0170R1, GG0170R2, G0170RR1, GG0170S1, GG0170S2, and GG0170SS1 must not be equal to [^].
c) If GG0170Q1=[-], then items GG0170R1, GG0170R2, G0170RR1, GG0170S1, GG0170S2, and GG0170SS1 must be equal to [-].
Version Notes

Item List
Item ID | Description
GG0170Q1 | Does patient use wheelchair and/or scooter (Adm)
GG0170R1 | Func Mobil (Adm Perf) - Wheel 50 feet w/2 turns
GG0170R2 | Func Mobil (Dschg Goal) - Wheel 50 feet w/2 turns
GG0170RR1 | Indicate type of wheelchair or scooter (Adm)
GG0170S1 | Func Mobil (Adm Perf) - Wheel 150 feet
GG0170S2 | Func Mobil (Dschg Goal) - Wheel 150 feet
GG0170SS1 | Indicate type of wheelchair or scooter (Adm)

Edit Summary | Previous edit | Next edit

NOTICE: These materials are in the public domain and cannot be copyrighted.
Generated: 03/16/2020 09:31:12 AM