-5066

Edit Summary | Previous edit | Next edit

Property | Specification
Data System

IRF-PAI
Data Specs V5.00.0 DRAFT
Edit Type Consistency
Severity Fatal
Edit Text a) If GG0170Q3=[0,^], then items GG0170R3, G0170RR3, GG0170S3, and GG0170SS3 must be equal to [^].
b) If GG0170Q3=[1], then items GG0170R3, G0170RR3, GG0170S3, and GG0170SS3 must not be equal to [^].
c) If GG0170Q3=[-], then items GG0170R3, G0170RR3, GG0170S3, and GG0170SS3 must be equal to [-].
Version Notes

Item List
Item ID | Description
GG0170Q3 | Does patient use wheelchair and/or scooter (Dschg)
GG0170R3 | Func Mobil (Dschg Perf) - Wheel 50 feet w/2 turns
GG0170RR3 | Indicate type of wheelchair or scooter (Dschg)
GG0170S3 | Func Mobil (Dschg Perf) - Wheel 150 feet
GG0170SS3 | Indicate type of wheelchair or scooter (Dschg)

Edit Summary | Previous edit | Next edit

NOTICE: These materials are in the public domain and cannot be copyrighted.
Generated: 03/16/2020 09:31:12 AM