-5085

Edit Summary | Previous edit | Next edit

Property | Specification
Data System

IRF-PAI
Data Specs V5.00.0 DRAFT
Edit Type Consistency
Severity Fatal
Edit Text (a) If GG0170I3=[07,09,10,88,^], then GG0170J3, GG0170K3 and GG0170L3 must equal [^].
(b) If GG0170I3=[06,05,04,03,02,01], then GG0170J3, GG0170K3 and GG0170L3 must not equal [^].
(c) If GG0170I3=[-], then GG0170J3, GG0170K3 and GG0170L3 must equal [-].
Version Notes

Item List
Item ID | Description
GG0170I3 | Func Mobil (Dschg Perf) - Walk 10 feet
GG0170J3 | Func Mobil (Dschg Perf) - Walk 50 feet w/2 turns
GG0170K3 | Func Mobil (Dschg Perf) - Walk 150 feet
GG0170L3 | Func Mobil (Dschg Perf) - Walk 10 Ft Uneven Surf

Edit Summary | Previous edit | Next edit

NOTICE: These materials are in the public domain and cannot be copyrighted.
Generated: 03/16/2020 09:31:12 AM