42

Item Summary | Previous item | Next item

Property | Specification
Data System

IRF-PAI
Data Specs V5.00.0 DRAFT
Description Program Interruption(s) Indicator
XML Tag R42
Group Asmt
Type Code
Length 1
Fixed Start-End 1005-1005
Version Notes

Item Values
Value | LOINC | Text
0 |  | No
1 |  | Yes

Item Edits
Edit ID | Type | Severity | Edit Text
-1115 | Consistency | Fatal | Inconsistent Skip Pattern: If Program Interruption(s) (42) is 0 (No), then the Program Interruption Dates (43A - 43F) must all be "No information" [^].
-1116 | Consistency | Fatal | Inconsistent 42/43A values: The Program Interruption(s) (42) value is not consistent with the 1st Interruption Date (43A) value. If Program Interruption(s) (42) is equal to 1 (Yes), then 1st Interruption Date (43A) must not be skipped with a value of "No information" [^].
-1010 | Format | Fatal | Invalid Data Value: The submitted value for this item is not in the valid range of acceptable values.

Item Summary | Previous item | Next item

NOTICE: These materials are in the public domain and cannot be copyrighted.
Generated: 03/16/2020 09:31:12 AM